| Messages

1391: THE REPORT MESSAGES

Used by the routine at MAIN_EXEC. Each message is given with the last character inverted (plus +80).
REPORTS | 1391 | DEFB $80 | Initial byte is stepped over.
| 1392 | DEFM "O","K"+$80 | 0 OK
| 1394 | DEFM "NEXT without FO","R"+$80 | 1 NEXT without FOR
| 13A4 | DEFM "Variable not foun","d"+$80 | 2 Variable not found
| 13B6 | DEFM "Subscript wron","g"+$80 | 3 Subscript wrong
| 13C5 | DEFM "Out of memor","y"+$80 | 4 Out of memory
| 13D2 | DEFM "Out of scree","n"+$80 | 5 Out of screen
| 13DF | DEFM "Number too bi","g"+$80 | 6 Number too big
| 13ED | DEFM "RETURN without GOSU","B"+$80 | 7 RETURN without GOSUB
| 1401 | DEFM "End of fil","e"+$80 | 8 End of file
| 140C | DEFM "STOP statemen","t"+$80 | 9 STOP statement
| 141A | DEFM "Invalid argumen","t"+$80 | A Invalid argument
| 142A | DEFM "Integer out of rang","e"+$80 | B Integer out of range
| 143E | DEFM "Nonsense in BASI","C"+$80 | C Nonsense in BASIC
| 144F | DEFM "BREAK - CONT repeat","s"+$80 | D BREAK - CONT repeats
| 1463 | DEFM "Out of DAT","A"+$80 | E Out of DATA
| 146E | DEFM "Invalid file nam","e"+$80 | F Invalid file name
| 147F | DEFM "No room for lin","e"+$80 | G No room for line
| 148F | DEFM "STOP in INPU","T"+$80 | H STOP in INPUT
| 149C | DEFM "FOR without NEX","T"+$80 | I FOR without NEXT
| 14AC | DEFM "Invalid I/O devic","e"+$80 | J Invalid I/O device
| 14BE | DEFM "Invalid colou","r"+$80 | K Invalid colour
| 14CC | DEFM "BREAK into progra","m"+$80 | L BREAK into program
| 14DE | DEFM "RAMTOP no goo","d"+$80 | M RAMTOP no good
| 14EC | DEFM "Statement los","t"+$80 | N Statement lost
| 14FA | DEFM "Invalid strea","m"+$80 | O Invalid stream
| 1508 | DEFM "FN without DE","F"+$80 | P FN without DEF
| 1516 | DEFM "Parameter erro","r"+$80 | Q Parameter error
| 1525 | DEFM "Tape loading erro","r"+$80 | R Tape loading error
COMMA_SPC | 1537 | DEFM ","," "+$80 | ', '