| Routines

1EA1: THE 'RUN' COMMAND ROUTINE

The address of this routine is found in the parameter table. The parameter of the RUN command is passed to NEWPPC by calling GO_TO. The operations of 'RESTORE 0' and 'CLEAR 0' are then performed before a return is made.
RUN | 1EA1 | CALL GO_TO | Set NEWPPC as required.
| 1EA4 | LD BC,$0000 | Now perform a 'RESTORE 0'.
| 1EA7 | CALL REST_RUN
| 1EAA | JR CLEAR_RUN | Exit via the CLEAR command routine.