| Routines

1076: THE 'ED-SYMBOL' SUBROUTINE

The address of this routine is derived from an offset found in the editing keys table.
Input
A | Code of the last key pressed
If SYMBOL and GRAPHICS codes were used they would be handled as follows:
ED_SYMBOL | 1076 | BIT 7,(IY+$37) | Jump back unless dealing with INPUT LINE (bit 7 of FLAGX set).
| 107A | JR Z,ED_ENTER
The address of this entry point is derived from an offset found in the editing keys table.
ED_GRAPH | 107C | JP ADD_CHAR | Jump back.