| Routines

09704: THE 'SCANNING BRACKET' ROUTINE

The address of this routine is derived from an offset found in the scanning function table.
S_BRACKET | 09704 | RST 32 | This routine simply gets the character and calls SCANNING recursively.
| 09705 | CALL SCANNING
| 09708 | CP ")" | Report the error if no matching bracket.
| 09710 | JP NZ,REPORT_C
| 09713 | RST 32 | Continue scanning.
| 09714 | JP S_CONT_2