| Messages

05009: THE REPORT MESSAGES

Used by the routine at MAIN_EXEC. Each message is given with the last character inverted (plus 128).
REPORTS | 05009 | DEFB 128 | Initial byte is stepped over.
| 05010 | DEFM "O","K"+128 | 0 OK
| 05012 | DEFM "NEXT without FO","R"+128 | 1 NEXT without FOR
| 05028 | DEFM "Variable not foun","d"+128 | 2 Variable not found
| 05046 | DEFM "Subscript wron","g"+128 | 3 Subscript wrong
| 05061 | DEFM "Out of memor","y"+128 | 4 Out of memory
| 05074 | DEFM "Out of scree","n"+128 | 5 Out of screen
| 05087 | DEFM "Number too bi","g"+128 | 6 Number too big
| 05101 | DEFM "RETURN without GOSU","B"+128 | 7 RETURN without GOSUB
| 05121 | DEFM "End of fil","e"+128 | 8 End of file
| 05132 | DEFM "STOP statemen","t"+128 | 9 STOP statement
| 05146 | DEFM "Invalid argumen","t"+128 | A Invalid argument
| 05162 | DEFM "Integer out of rang","e"+128 | B Integer out of range
| 05182 | DEFM "Nonsense in BASI","C"+128 | C Nonsense in BASIC
| 05199 | DEFM "BREAK - CONT repeat","s"+128 | D BREAK - CONT repeats
| 05219 | DEFM "Out of DAT","A"+128 | E Out of DATA
| 05230 | DEFM "Invalid file nam","e"+128 | F Invalid file name
| 05247 | DEFM "No room for lin","e"+128 | G No room for line
| 05263 | DEFM "STOP in INPU","T"+128 | H STOP in INPUT
| 05276 | DEFM "FOR without NEX","T"+128 | I FOR without NEXT
| 05292 | DEFM "Invalid I/O devic","e"+128 | J Invalid I/O device
| 05310 | DEFM "Invalid colou","r"+128 | K Invalid colour
| 05324 | DEFM "BREAK into progra","m"+128 | L BREAK into program
| 05342 | DEFM "RAMTOP no goo","d"+128 | M RAMTOP no good
| 05356 | DEFM "Statement los","t"+128 | N Statement lost
| 05370 | DEFM "Invalid strea","m"+128 | O Invalid stream
| 05384 | DEFM "FN without DE","F"+128 | P FN without DEF
| 05398 | DEFM "Parameter erro","r"+128 | Q Parameter error
| 05413 | DEFM "Tape loading erro","r"+128 | R Tape loading error
COMMA_SPC | 05431 | DEFM ","," "+128 | ', '