| Data

15C6: THE 'INITIAL STREAM DATA'

Used by the routines at NEW and CLOSE. Initially there are seven streams - +FD to +03.
STRMDATA | 15C6 | DEFW $0001 | +FD: Leads to channel 'K' (keyboard)
| 15C8 | DEFW $0006 | +FE: Leads to channel 'S' (screen)
| 15CA | DEFW $000B | +FF: Leads to channel 'R' (work space)
| 15CC | DEFW $0001 | +00: Leads to channel 'K' (keyboard)
| 15CE | DEFW $0001 | +01: Leads to channel 'K' (keyboard)
| 15D0 | DEFW $0006 | +02: Leads to channel 'S' (screen)
| 15D2 | DEFW $0010 | +03: Leads to channel 'P' (printer)