| Routines

04108: THE 'CURSOR RIGHT EDITING' SUBROUTINE

The address of this routine is derived from an offset found in the editing keys table.
Input
HL | Address of the cursor (K-CUR)
ED_RIGHT | 04108 | LD A,(HL) | The current character is tested and if it is 'carriage return' then return.
| 04109 | CP 13
| 04111 | RET Z
| 04112 | INC HL | Otherwise make the cursor come after the character.
This entry point is used by the routine at ED_LEFT.
ED_CUR | 04113 | LD (23643),HL | Set the system variable K-CUR.
| 04116 | RET |