| Routines

B1E8: Print a character's title and name, and walk him onto the screen (2)

Continues from B0E8. Prints the character's name followed by a space.
Input
B | 1-8 (corresponding to one of the eight main characters)
HL | Message address for the character's name
B1E8 | PUSH BC |
B1E9 | LD DE,$5020 | This is the display file address at which to print the character's name
B1EC | CALL $AFE8 | Print the character's name
B1EF | LD HL,$B477 | B477: ' '
B1F2 | CALL $B3F9 | Print a space
B1F5 | LD HL,$9860 | Point HL at byte 0x60 of little boy no. 1's buffer
B1F8 | POP BC |
B1F9 | LD A,B | A=1-8 (corresponding to one of the eight main characters)
B1FA | NOP |
B1FB | NOP |
B1FC | JP $B2E8 |